from gpiozero import LED

from time import sleep

led = LED(4) # gpio 4 board number 7 connect c7 to c20

while True:

led.on()

sleep(1)

led.off()

sleep(1)